
	[YOUR HANDYMAN BUSINESS]

	HOME MAINTENANCE CHECKLIST

	What to check every month, every season and once a year — check it off, date it, and pass the big jobs to a pro

	Home: ______________________________ Year: ________ Built in: ________

	Filter size: __________ Water shut-off: __________________ Breaker panel: __________

	EVERY MONTH

	☐
	Press the test button on every smoke and carbon monoxide alarm

	☐
	Look at the furnace or AC filter — change it when it's gray

	☐
	Run water in sinks and tubs nobody uses, and flush those toilets

	☐
	Look under every sink for drips and soft cabinet floors

	☐
	Clean the range hood filter and the garbage disposal

	☐
	Press test and reset on every GFCI outlet

	SPRING

	☐
	Clear the gutters and point every downspout away from the house

	☐
	Book the air conditioning check-up before the first hot week

	☐
	Look at the roof from the ground: missing, curled or lifted shingles

	☐
	Turn on the outside faucets and check for leaks after the freeze

	☐
	Walk the deck and the steps for loose boards and raised nails

	SUMMER

	☐
	Clean the dryer vent duct, and check the hood outside flaps open

	☐
	Trim branches and shrubs back from the roof and the walls

	☐
	Look in the attic for daylight, damp patches and nests

	☐
	Check the caulk around tubs, showers, sinks and windows

	FALL

	☐
	Clear the gutters again once the leaves are down

	☐
	Book the furnace check-up before the first cold night

	☐
	Shut off and drain the outside faucets; bring the hoses in

	☐
	Check the weatherstripping and the door sweeps for daylight

	☐
	Have the chimney looked at before the first fire

	☐
	Seal the gaps where pipes and wires come through the walls

	WINTER

	☐
	Keep snow off the dryer vent, the furnace vent and the meter

	☐
	Watch the roof edge for ice dams and long icicles

	☐
	Check pipes in the garage, crawl space and outside walls

	☐
	Look around the water heater for drips and rust

	ONCE A YEAR

	☐
	Put new batteries in every 9-volt smoke alarm, and the backup battery in hardwired ones

	☐
	Read the date on the back of each smoke alarm — 10 years old means a new one

	☐
	Drain or flush the water heater as its manual says

	☐
	Vacuum the refrigerator coils

	☐
	Test the sump pump: pour in a bucket of water and watch it run

	☐
	Check the fire extinguisher gauge reads in the green

	☐
	Walk the outside: peeling paint, cracked siding, gaps in the foundation

	☐
	Test the garage door: it should stop and reverse when it meets something

	JOBS FOR A PRO

	Job: ________________________ Who: ________________ Booked: ______ Done: ______

	Job: ________________________ Who: ________________ Booked: ______ Done: ______

	Job: ________________________ Who: ________________ Booked: ______ Done: ______

	Job: ________________________ Who: ________________ Booked: ______ Done: ______

	Gas lines, the breaker panel and new circuits usually go to a licensed trade. The rest can wait for one handyman visit with the whole list.

	Write the date next to each check mark. A checklist with dates is the one that tells you the gutters were last cleared in May — and something a new handyman or a buyer's inspector may ask about.

	[Your handyman business] · [Your phone] · [Your website]



Free from zarla.com/guides/home-maintenance-checklist. Replace every [bracketed] line. Put the seasonal checklist on your website, and quote and invoice the visit from the same place: zarla.com/website-builder/handyman
